;***********************************************************************
; SE4501D.INF
;
;   This installation script supports Windows 98, Me, 2000 and XP for  ;   Gigaset USB Adapter 54.
;   Gigaset USB Adapter 54
;   Copyright 2001-2003 Siemens. 
;   All Rights Reserved.
;
;***********************************************************************

[Version]
 DriverVer = 03/22/2004, 1.0.9.2
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
; CatalogFile         = SE4501D.cat
; MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList,NTx86.5.1

[DeviceList]
 %A021_DESC_STR%     = PRISM_A021,        USB\VID_083A&PID_4502

[DeviceList.NTx86.5.1]
 %A021_DESC_STR%     = PRISM_A021_XP,        USB\VID_083A&PID_4502

;==========================================
[PRISM_A021]       ; Win9x
 AddReg         = PRISM_A021.reg, PRISM_DCB1.reg1, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_CCU.copy

;[PRISM_A021.ME]    ; WinMe
; AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
; CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_CCU.copy

;[PRISM_A021.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
; AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
; CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_CCU.copy

[PRISM_A021.NT]    ; Win2k
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_CCU.copy
 BusType        = 0
 Characteristics= 0x84

[PRISM_A021.NT.Services]
 AddService= "SE4501D", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[PRISM_A021.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_A021_XP]    ; Winxp
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.XP, PRISM_CCU.copy
 BusType        = 0
 Characteristics= 0x84

[PRISM_A021_XP.Services]
 AddService= "SE4501D", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[PRISM_A021_XP.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT 

[PRISM_DCB1.reg1]
; HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce, "SE4501D",, "%11%\CCU4501D.exe"

[PRISM_A021.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_083A&PID_4502"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A021_DESC_STR%
 HKR,,CountryCode,0,"DE "
 HKR,,11dMode,0,0
 HKR,,EnableRadio,0,1
 HKR,,CCUEnable,0,1

;if have ccu ,CountryCode add (HKR,,CountryCode,0,"DE ")
;11dMode all add (HKR,,11dMode,0,0)
;if have ccu EnableRadio set 0 ,have no ccu set 1
;if have ccu CCUEnable set 0 ,have no ccu set 1

 
;###############################################################################
[PRISM_COINSTALL.reg.NT]
; HKR,           ,CoInstallers32         ,0x00010000     ,"CCU4501D.dll,CoDCSUup"

[PRISM_DRIVER_A02.Service]
 DisplayName    = %A02_SERVICE_STR%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\SE4501D.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_A02.reg]
 HKR,NDI                ,Service                ,0      ,"SE4501D"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"
 HKR,                   ,DeviceVxDs             ,0      ,"SE4501D.sys"

[COMMON_NDIS.reg]
; Win9X
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"SE4501D"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"SE4501D"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
 HKR,			,NitroMode		,0	,"1"
 HKR,			,NitroTime		,0	,"650"
;Uncomment the line above to install without user interface prompts


 HKR,Ndi\params\RTSThresh,default,0,"2347"
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,"int"
 HKR,NDI\params\RTSThresh,flag,1,"20","00","00","00"
 HKR,NDI\params\RTSThresh,min,0,"0"
 HKR,NDI\params\RTSThresh,max,0,"2347"
 HKR,NDI\params\RTSThresh,step,0,"1"
;; HKR,NDI\params\RTSThresh,optional,0,"1"

 HKR,Ndi\params\FragThresh,default,0,"2346"
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,"int"
 HKR,NDI\params\FragThresh,flag,1,"20","00","00","00"
 HKR,NDI\params\FragThresh,min,0,"256"
 HKR,NDI\params\FragThresh,max,0,"2346"
 HKR,NDI\params\FragThresh,step,0,"2"
 ;;HKR,NDI\params\FragThresh,optional,0,"1"


 HKR,NDI\params\ShortRetryLimit,default,0,"7"
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,"int"
 HKR,NDI\params\ShortRetryLimit,min,0,"1"
 HKR,NDI\params\ShortRetryLimit,max,0,"255"
 HKR,NDI\params\ShortRetryLimit,step,0,"1"
;; HKR,NDI\params\ShortRetryLimit,optional,0,"1"


 HKR,NDI\params\LongRetryLimit,default,0,"4"
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,"int"
 HKR,NDI\params\LongRetryLimit,min,0,"1"
 HKR,NDI\params\LongRetryLimit,max,0,"255"
 HKR,NDI\params\LongRetryLimit,step,0,"1"
 ;;HKR,NDI\params\LongRetryLimit,optional,0,"1"


 HKR,NDI\params\ConfigProfile,default,0,"1"
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,,"enum"
 HKR,NDI\params\ConfigProfile,flag,1,"20","00","00","00"
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 ;;HKR,NDI\params\ConfigProfile,optional,0,"1"

 ;HKR,NDI\params\NitroMode,default,0,"1"
 ;HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 ;HKR,NDI\params\NitroMode,type,,"enum"
 ;HKR,NDI\params\NitroMode,flag,1,"20","00","00","00"
 ;HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 ;HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 ;;HKR,NDI\params\NitroMode,optional,0,"1"

 
 HKR,Ndi\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,"enum"
 HKR,NDI\params\PSMode,flag,1,"20","00","00","00"
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 ;;HKR,NDI\params\PSMode,optional,0,"1"

  HKR,NDI\params\PpePdlpEnable,default,0,"1"
 HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
 HKR,NDI\params\PpePdlpEnable,type,,"enum"
 HKR,NDI\params\PpePdlpEnable,flag,1,"20","00","00","00"
 HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%
 ;;HKR,NDI\params\PpePdlpEnable,optional,0,"1"

 HKR,NDI\params\PpeCompressEnable,default,0,"1"
 HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
 HKR,NDI\params\PpeCompressEnable,type,,"enum"
 HKR,NDI\params\PpeCompressEnable,flag,1,"20","00","00","00"
 HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%
 ;;HKR,NDI\params\PpeCompressEnable,optional,0,"1"

 HKR,NDI\params\PpeConcatEnable,default,0,"1"
 HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
 HKR,NDI\params\PpeConcatEnable,type,,"enum"
 HKR,NDI\params\PpeConcatEnable,flag,1,"20","00","00","00"
 HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%
 ;;HKR,NDI\params\PpeConcatEnable,optional,0,"1"

 HKR,NDI\params\PpePiggyBackEnable,default,0,"1"
 HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
 HKR,NDI\params\PpePiggyBackEnable,type,,"enum"
 HKR,NDI\params\PpePiggyBackEnable,flag,1,"20","00","00","00"
 HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%
 ;;HKR,NDI\params\PpePiggyBackEnable,optional,0,"1"



;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers
 PRISM_DRIVER.copy.XP   = 12 ; Win2k=%windir%\system32\drivers
; PRISM_CCU.copy		= 11 ; Win9x=%windir%\system

[PRISM_CCU.copy]
;  CCU4501D.exe

[PRISM_DRIVER.copy]
; SE4501D.sys

[PRISM_DRIVER.copy.ME]
; SE4501D.sys

[PRISM_DRIVER.copy.NT]
; SE4501D.sys

[PRISM_DRIVER.copy.XP]
; SE4501D.sys,SE4501D1.sys,,

[PRISM_COINSTALL.copy.NT]
; CCU4501D.dll

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 SE4501D.sys           = 1
; CCU4501D.exe		= 1

[SourceDisksFiles.ME]   ; WinMe
 SE4501D.sys           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 SE4501D.sys           = 1
 SE4501D1.sys		= 1
; CCU4501D.dll		= 1
; CCU4501D.exe		= 1

;###############################################################################
[Strings]
;String ID               = String Text
;---------                 -----------
 VER_VENDOR_STR          = "Siemens AG"
 VER_VENDOR_NAME_STR     = "Siemens AG"
 INSTALL_DISK_STR        = "Gigaset USB Adapter 54 Driver Install Disk"


 A021_DESC_STR           = "Gigaset USB Adapter 54"
 A02_SERVICE_STR         = "Gigaset USB Adapter 54 Driver"

 ON_STR                  = "On"
 OFF_STR                 = "Off"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 ;NITRO_MODE              = "Nitro Mode"
  PPE_PDLP                = "Direct Link"
 PPE_COMPRESS            = "Compression"
 PPE_CONCAT              = "Concatenation"
 PPE_PIGGYBACK           = "PiggyBack"


