;################################################################################
;
;
;  Name:	  		rtgbodi.100
;             		
;  Version:	  		V1.00
;
;  Released By:   	ken
;                 	
;  Release Date:  	6/6/02
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  
;		
;  Comment:       
;                 
;################################################################################ 
;  Name:	  		rtgbodi.101
;             		
;  Version:	  		V1.01
;
;  Released By:   	ken
;                 	
;  Release Date:  	11/25/02
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  		low performance for the Half-duplex
;		
;  Comment:       
;                 
;################################################################################        
;  Name:	  		rtgbodi.102
;             		
;  Version:	  		V1.02
;
;  Released By:   	ken
;                 	
;  Release Date:  	6/26/03
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  		Add the PHY parameter for the 8110
;		
;  Comment:       
;                 
;################################################################################        
;  Name:	  		rtgbodi.103
;             		
;  Version:	  		V1.03
;
;  Released By:   	ken
;                 	
;  Release Date:  	7/15/03
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  		tsi-twi issue
;		
;  Comment:       
;                 
;################################################################################        
;  Name:	  		rtgbodi.104
;             		
;  Version:	  		V1.04
;
;  Released By:   	ken
;                 	
;  Release Date:  	7/18/03
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  		check the PHY version (0 or 1) 
;		
;  Comment:       
;                 
;################################################################################        
;  Name:	  		rtgbodi.105
;             		
;  Version:	  		V1.05
;
;  Released By:   	ken
;                 	
;  Release Date:  	9/4/03
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  		incompatible for the server RTL8029 driver (10M)
;		
;  Comment:       
;                 
;################################################################################        
;  Name:	  		rtgbodi.106
;             		
;  Version:	  		V1.06
;
;  Released By:   	ken
;                 	
;  Release Date:  	4/5/04
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  		modify the PHY parameter for .13 B
;		
;  Comment:       
;                 
;################################################################################       
;  Name:	  		rtgbodi.107
;             		
;  Version:	  		V1.07
;
;  Released By:   	ken
;                 	
;  Release Date:  	7/1/04
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  		modify the PHY parameter for .13 C
;		
;  Comment:       
;                 
;################################################################################      
;  Name:	  		rteodi.108
;             		
;  Version:	  		V1.08
;
;  Released By:   	Vika Yen
;
;  Release Date:  	08/04/05
;
;  Changed File:  	rteodi.asm
;
;  Reason:	  		Release RTL8168B Novell Client Driver
;		
;  Comment:    
;		  			1.  Driver incrase to recognize RTL810X family
;		  			2.  Disable Gigabit capability
;		  
;############################################################################   
;  Name:	  		rtgbodi.109
;             		
;  Version:	  		V1.09
;
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	09/08/05
;                 	
;  Changed File:  	rtgbodi.asm
;                 	
;
;  Reason:	  		RTL8110SBL RMA issue
;		
;  Comment:    
;		  			1.  Fix the power-saving problem in RTL8169SBL
;		
;############################################################################   
;  Name:	  		rtgbodi.110
;             		
;  Version:	  		V1.10
;
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	01/23/06
;                 	
;  Changed File:  	rtgbodi.asm
;
;
;  Reason:	  
;		
;  Comment:    
;				   	1. Support for RTL8169SC
;				   	2. Support for RTL8101E
;				   	3. Add pactch tool that support RTL8169/8168/810XE serial
;				   	4. Adjust number of TCB's this Module will allocate be "8" in Ethertsm.asm	  
;				   	5. Modify PCIE adapter multicast register order be : MAR7~MAR0
;				   	6. Increase check reset nic condition that no TOK to created.	
;				   
;############################################################################  
;  Name:	      	rtgbodi.111
;                 	
;  Version:	  	  	V1.11
;                 	
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	02/14/06
;                 	
;  Changed File:  	rtgbodi.asm
;
;
;  Reason:	  
;		
;  Comment:    
;				   	1. Change RTL8110SC DID to "8167"
;				   	2. Resolve interrupt issue at some platforms
;############################################################################  
;  Name:			rtgbodi.112
;
;  Version:	  	  	V1.12
;
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	02/24/06
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  	  
;		
;  Comment:    
;				  	1. Modify parameter with RTL8100E
;						2. Adjust PHY Parameters of RTL8169/RTL8168/RTl810XE serials
;############################################################################ 
;  Name:						rtgbodi.113
;
;  Version:	  	  	V1.13
;
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	05/22/06
;                 	
;  Changed File:  	rtgbodi.asm
;
;  Reason:	  	  
;		
;  Comment:    
;				  			1.	Modify PHY Parameters of RTL8169S
;								2.	Display correctly MAC Address with Multi-Adapters
;############################################################################         
;  Name:						rtgbodi.114
;
;  Version:	  	  	V1.14
;
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	09/12/06
;                 	
;  Changed File:  	rtgbodi.asm,MSM.ASM,DRIVER.INC,MSMTXT.INC
;
;  Reason:	  	  
;		
;  Comment:    
;				  			    1. Modify PHY Parameters of RTL8169S
;                   2. Modify PHY Parameters of PCIE adapters
;                   3. Support upper memory
;                   4. Support indicating specific card to load ODI driver.
;############################################################################       


