;************************************************************************
;*
;*  Chapter 1. How to use this patch file?
;*
;*      This file (RPL.TXT) contains info. that helps you patch
;*      'RPL.ROM'(v1.00) file into your own Boot ROM driver.
;*
;*      To generate your custom driver, please follow the steps
;*      described below:
;*
;*      a). Follow the instructions to edit the message area in each
;*          line. Save this file when you finish editing.
;*          ( see CHAPTER 2 for more details ! )
;*
;*         !!! NOTE: DO NOT EDIT THE OFFSET AND LENGTH AREA !!!
;*
;*      b). Make sure that you have the following files in your working
;*          directory:
;*
;*              RTPATCH.EXE ------->   The patch execution file
;*		ROMCKSUM    ------->   ROM checksum calculate utilty
;*              RPL.ROM     ------->   ROM image file
;*              RPL.TXT     ------->   ROM patch info. file
;*
;*      c). After you decide the name for your RPL ROM,
;*          simply type:
;*
;*          > RTPATCH RPL.ROM RPL.TXT  [your ROM]  <Enter> 
;*
;*         !!! NOTE: DO NOT USE THE SAME DRIVER NAME AS THE ORIGINAL
;*                   DRIVER!!!
;*
;*      d). Then, re-check romsum to your own ROM
;*          just type:
;*
;*           ROMCKSUM   -romsize=12k  -cksum=7 [your ROM]  <ENTER>
;*
;*
;*      e). If no error occurs, you should find your custom driver is
;*          generated under your working directory.
;*
;*
;* Chapter 2. How to edit this file ?
;*
;*
;*      Each line in this file contains a display message info. of the
;*      driver. Each line has the same format:
;*
;*          <offset> <length> <message>
;*      e.g.
;*           1266      28      'Packet driver for RTL8129',0dh,0ah,'$';
;*           ----      --      ----------------------------------------
;*                                                                
;*        Do not edit here!       |                                 | EOL
;*                           Put your own message here!           |
;*          (HEX)     (DEC)                                     delimiter
;*
;*
;*
;*      *NOTE: DO NOT EDIT THE <offset> AND <length> AREA !!!
;*
;*      *NOTE: Anything after comment character ';' will be ignored!
;*
;*      *NOTE: Always add ';'(EOL) at end of each line!
;*
;*      *NOTE: If delimiter is needed, keep delimiter intact! In this case,
;*             leave the '$' as the last byte.
;*
;*      *NOTE: 0H can only be added as delimiter! Message after 0H will be lost!
;*
;*      *NOTE: Total length of your message should not exceed <length>.
;*
;*      *NOTE: If you must use the comment character (;) in your message,
;*             put 3bh instead of ';'. Same for (').
;*
;*      *NOTE: Do not exceed 250 characters in each line.
;*
;************************************************************************


;************************************************************************
;       Put RPL driver name here
;************************************************************************

518  2  ech,10h;	;Vendor ID
51a  2  69h,81h;	;Device ID

1b42 1   07h
1b43 9   'RTGBODI',0h
2539 8   'RTGBODI'

78d  20	 'Realtek Corporation',0h
7a1  12	 'Realtek RPL',0h
17cd 48  'Realtek RTL8169S/RTL8110S Gigabit RPL BootROM',0dh,0ah,0h
1895 33	 'Realtek Bootstrap selection menu',0h 

1b0e 52  32h,'Realtek RTL8169/8110 Family Gigabit Ethernet      ',0h;
249f 142 'Realtek RTL8169/8110 Family Gigabit Ethernet MLID  v1.07 (09-09-04) ',0dh,0ah,'(c) Copyright 2003, by Realtek Semiconductor Corp. All rights reserved.',0h;

